


**IP DHCP (HELPER-ADDRESS)**


**Routing is neccesary to assign ip through one dhcp server**


****


**Router 1**





**PC 1**

**Router 2**



**PC 2 (if dhcp failed try “ip dhcp –d” command on PC)**

**Router 3**



**PC 3**

